RPMTorque=( 0.0, -21.5, -21.5)
RPMTorque=( 500.0, -23.4, 63.4)
RPMTorque=( 1000.0, -25.3, 124.8)
RPMTorque=( 1500.0, -28.0, 156.4)
RPMTorque=( 2000.0, -30.6, 181.7)
RPMTorque=( 2500.0, -32.6, 205.8)
RPMTorque=( 3000.0, -36.2, 226.2)
RPMTorque=( 3500.0, -39.5, 238.6)
RPMTorque=( 4000.0, -47.7, 247.4)
RPMTorque=( 4500.0, -55.0, 252.9)
RPMTorque=( 5000.0, -60.3, 257.3)
RPMTorque=( 5500.0, -69.6, 254.0)
RPMTorque=( 6000.0, -78.6, 237.5)
RPMTorque=( 6500.0, -88.4, 211.3)
RPMTorque=( 7000.0, -98.8, 188.2)
RPMTorque=( 7500.0, -110.7, 159.8)
RPMTorque=( 8000.0, -124.2, 131.3)
RPMTorque=( 8500.0, -138.1, 90.7)
RPMTorque=( 9000.0, -153.0, 42.5)
RPMTorque=( 9500.0, -166.9, -14.6)
RPMTorque=( 10000.0, -179.2, -78.0)
RPMTorque=( 10500.0, -189.9, -132.7)
FuelConsumption=4.400e-005          // affected by throttle position and engine speed
FuelEstimate=1.020                  // fudge factor for differences between vehicle types (used for lap estimates and AI pit scheduling)
EngineInertia=0.1725
IdleThrottle=0.75
IdleRPMLogic=(1000.0, 1300.0)
LaunchEfficiency=0.000              // efficiency (0.0-1.0) of launch control, or 0.0 if N/A
LaunchRPMLogic=(3000.0, 4000.0)     // holds RPM in this range before launch (used for AI even if launch control is N/A!)
RevLimitRange=(7500.0, 100.0, 1)
RevLimitSetting=0
RevLimitLogic=150.0                 // RPM range around current setting where rev limiter operates
EngineMapRange=(0, 1, 1)            // 0 = most driveable, max = most power (low gears only) (unimplemented)
EngineMapSetting=0
EngineBrakingMapRange=(0.0, 0.001, 1) // input throttle is ranged from minimum to 100%, with the minimum = setting * step * RPM,
EngineBrakingMapSetting=0             // i.e. if you want 10% throttle at 6000 RPM, set the middle number to 10/6000 = 0.00167
OptimumOilTemp=100.5                // degrees Celsius at which engine operates optimally
CombustionHeat=41.0                 // degrees Celsius added per liter of fuel burned
EngineSpeedHeat=8.000e-004          // heat added linearly with engine speed
OilMinimumCooling=7.500e-003        // heat dissipated without oil/water transfer
OilWaterHeatTransfer=(3.900e-001,7.900e-005)  // heat transfer from oil to water (base, w/ engine speed)
WaterMinimumCooling=4.000e-003      // base heat dissipated without velocity
RadiatorCooling=(1.780e-006, 4.510e-006)      // cooling rate with velocity (base, per setting)
LifetimeEngineRPM=(11770.0,180.0)   // (base engine speed for lifetime, range where lifetime is halved)
LifetimeOilTemp=(108.0,2.50)        // (base oil temp for lifetime, range where lifetime is halved)
LifetimeAvg=15000                   // average lifetime in seconds
LifetimeVar=5500                    // lifetime random variance
EngineEmission=(0.20, 0.60, -2.5)   // where flames and smoke are emitted (relative to ref frame at rear axle)
EngineSound=(0.20, 0.60, -2.5)      // where engine sound is emitted (relative to ref frame at rear axle)
SpeedLimiter=1                      // whether there is a pitlane speed limiter
OnboardStarter=1                    // whether vehicle restarts when stalled
StarterTiming=(1.5, 0.0, 0.0)       // average and variable cranking time, then blend with starting sound

